| RevealEarth - True Color Elevations v2.5 Demo Quick Tutorial |
| Content Demo Quick Tutorial Run Run the Demo Examine Data by Pixel Apply Visual Data Filters View 3D Elevation Plots Export Elevation Data Add User Notes Contact Us Demo Quick Tutorial This demonstration contains a small portion of global imagery. To view complete image (global 1KM resolution, at 21600X43200 pixel) with index features (e.g. Zoom In/Out, Go to), please purchase RevealEarth-True Color Elevations RevealEarth - True Color Elevations does not require installation. Simply start the RevealEarth browser by double-clicking RvlEarth.exe. You will need MS Windows 98/NT/2000/Me/XP. Follow the steps below for a quick tour of some browser features. Run the DemoRevealEarth - True Color Elevations 1. Double-click "RvlEarth.exe" to start the RevealEarth browser. 2. Click the "Open ..." button, a dialog box appears. 3. Select "Remote Sensing" from the "Main category list", select "Elevation - True color" from the "Sub category list" and click OK, a window opens to display image. Examine Data by Pixel 4. Click the Image Pixel button. 5. Move your cursor to any point of interest on the image, the "Image Pixel" dashboard appearing at the lower right corner of the image window displays the elevation data value for the current pixel. Apply Visual Data Filters 6. Choose a pixel of moderate elevation with respect to its surroundings. 7. Right-click the target pixel, a pop-up menu appears. 8. Select "Image Filter On", an "Image Filter" dialog box appears. 9. Choose "Interpreted Elevation (m)" from the "Analysis by" section, "Above" from "Select target range", "No filter" from "Luminosity filter", and "Highlight target area" from "Filter display style", then click OK, all pixels of elevations greater than your target will be highlighted to a transparent color. 10. Right-click the image again and select "Image Filter Off". View 3D Elevation Plots 11. Continuing at this image level, locate a region of interest. Right-click for 3D visualization and a pop-up menu appears. 12. Select "Image 3D Study", a dialog box appears for you to choose between two 3D modes "Quick browse" and "High quality". 13. Select "Quick browse" and click OK. A new window appears to display an interactive 3D plot of the target region. 14. Position your cursor over the source image, drag with the right mouse button to refresh the 3D plot with data from a new location. 15. Right click on the source image and choose "Image 3D Study" again, this time select "High quality" mode. 16. Position your cursor over the 3D image, drag with the left mouse button to alter viewing angle. 17. Use your mouse scroll wheel to increase/decrease the size of your 3D plot. 18. Reduce or increase vertical magnification if necessary via the horizontal scroll bar. 19. Right-click over the 3D image and choose "Select 3D Options" , the "Select 3D options" dialog box appears. 20. Select "False color" and OK to have elevations represented by a color sequence. A localized false color scheme will be applied to the plotted region, which dynamically maps the span of local elevation values across the entire false color set, to effectively illustrate elevation patterns even in flatter areas. 21. You can make other changes in the 3D display options to meet your requirement. For example, select 3 in the "Surface color smoothing coefficient" drop down box to improve visualization smoothness. Export Elevation Data 22. Right-click over the 3D image and choose "Data Export", the "Export Elevation Data Options" dialog box appears. 23. Select "Tab delimited" and keep "Include header information" checked, and click OK. 24. Click OK again in the Message box. 25. Open a new Excel file and select "Paste" from the "Edit" menu to obtain elevation data for your current 3D plot. Add User Notes 26. Close the 3D visualization window, and maximize the source image. 27. From the tools menu, select "Set User Note". 28. Place your cursor over a location you might wish to revisit and left click, a dialog box appears. 29. Enter a label for this location in the "Note index" field, and some comments in the "Note" field, then click OK. Your note will be added with a marker and the label you specified on the image. 30. Add one or two other notes at other places in the world. 31. Using the Find feature, select the Note/Track option, and you will find a list of all the notes you have made. Choose one to revisit, and click OK. 32. Your note marker will now appear at the center of the screen, click directly on the symbol (when the cursor becomes a question mark). The note's data is displayed, and can be modified. 33. From the Tools menu, select "Save", a dialog box appears. Name the file "test notes" for example, and save your data onto your computer (the file will be saved with the .mnt extension). 34. From the Tools menu again, select "Exit Notes/Track". And you will have left the Notes mode. 35. You can open your file using the "Open Note/Track File" feature under the Tools menu, which will re-populate the system with your notes (use Find to locate your notes if needed). 36. The User Track feature operates the same as User Notes. Lines will join each note you add to convey sequential order. (Insertions/modifications involving sequence changes can be made by directly editing your .mnt file using Notepad). Contact Us If you have questions, please contact us at support@inforshell.com Copyright © 2005-2006 InforShell Technologies, Inc. All rights reserved. Back to the top |